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2 МП фиксированная миниатюрная цилиндрическая IP-камера с ИК-подсветкой
IPC2122LB-AF28(40)-ECO2
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Features	
· High quality image with 1080P, 1/3.0" CMOS sensor
· 1080P (1920 × 1080)@30/25 fps; 720P (1280 × 720)@30/25 fps
· Supports accurate human body detection 2.0
· Ultra 265, H.265, H.264
· 2D/3D DNR (digital noise reduction)
· ROI (region of interest) ensures image quality in areas of interest with low bandwidth
· Smart IR, up to 30 m (98.4 ft.) IR distance
· Built‑in mic
· Wide temperature range: ‑30 ℃ to 60 ℃ (‑22 ℉ to 140 ℉)
· Supports PoE power supply
· IP67
Specifications	
	Model
	IPC2122LB‑AF28‑ECO2
	IPC2122LB‑AF40‑ECO2

	Camera

	Max Resolution
	2 MP

	Sensor
	1/3.0" CMOS

	Min. Illumination
	Color: 0.01 Lux (F2.0, AGC ON), 0 Lux with IR on

	Day/Night
	IR‑cut filter with auto switch (ICR)

	Shutter
	Auto/Manual, 1 to 1/100000 s

	Adjustment Angle
	Pan: 0° to 360°, Tilt: 0° to 90°, Rotate: 0° to 360°

	S/N
	> 52 dB

	WDR
	DWDR

	Lens

	Focal Length
	2.8 mm
	4.0 mm

	Iris
	F2.0

	Field of View (H)
	87.8 °
	67.3 °

	Field of View (V)
	48.9 °
	37.2 °

	Field of View (D)
	99.0 °
	77.8 °

	Lens Type
	Fixed

	Iris Type
	Fixed

	DORI

	DORI Distance (Lens)
	2.8 mm
	4.0 mm

	DORI Distance (Detect)
	51.4 m (168.7 ft.)
	73.5 m (241.0 ft.)

	DORI Distance (Observe)
	20.6 m (67.5 ft.)
	29.4 m (96.4 ft.)

	DORI Distance (Recognize)
	10.3 m (33.8 ft.)
	14.7 m (48.2 ft.)

	DORI Distance (Identify)
	5.1 m (16.9 ft.)
	7.3 m (24.1 ft.)

	Illuminator

	Illumination Distance (IR)
	30 m (98.4 ft.)

	Wavelength
	850 nm

	IR On/Off Control
	Auto/Manual

	Supplemental Light
	IR

	Video

	Video Compression
	Ultra 265, H.265, H.264

	H.264 Code Profile
	Baseline profile, Main profile, High profile

	Frame Rate
	Main Stream: 1080P (1920 × 1080), max. 30 fps
Sub Stream: 640 × 360, max. 30 fps; 2CIF (704 × 288), max. 30 fps; CIF (352 × 288), max. 30 fps;

	Video Bit Rate
	128 Kbps to 6144 Kbps

	U‑code
	Support

	OSD
	Up to 4 OSDs

	Privacy Mask
	Up to 4 areas

	Snapshot
	N/A

	ROI
	Up to 8 areas

	Video Stream
	Dual streams

	Image

	Smart IR
	Support

	White Balance
	Auto, Outdoor, Fine tune, Sodium lamp, Locked, Auto2

	Digital Noise Reduction
	2D/3D DNR

	Flip
	Normal, Flip vertical, Flip horizontal, 180°

	Dewarping
	N/A

	HLC
	Support

	BLC
	Support

	Defog
	Digital defog

	Events

	Basic Detection
	Motion detection, Audio detection, Human body detection 2.0

	General Function
	Watermark, IP address filtering, Access policy, ARP protection, RTSP authentication, User authentication, HTTP authentication

	Audio

	Audio Compression
	G.711U, G.711A

	Audio Bitrate
	64 Kbps

	Two‑way Audio
	N/A

	Suppression
	Support

	Sampling Rate
	8 kHz

	Storage

	Edge Storage
	N/A

	Network

	Protocols
	IPv4, IGMP, ICMP, ARP, TCP, UDP, DHCP, RTP, RTSP, DNS, DDNS, NTP, UPnP, HTTP, QoS, RTCP, RTMP

	Compatible Integration
	API, SDK

	Client
	EZStation, APP

	Web Browser
	Plug‑in required live view: IE 10+, Chrome 45+, Firefox 52+, Edge 79+, Plug‑in free live view: Chrome 57+, Firefox 58+, Edge 16+

	Security
	Password protection, Strong Password, Export operation logs, Basic and Digest Authentication for RTSP, Digest Authentication for HTTP, WSSE and Digest Authentication for ONVIF

	User/Host
	Up to 32 users. 2 user levels: administrator and common user

	Interface

	Audio I/O
	N/A

	Alarm I/O
	N/A

	Serial Port
	N/A

	Built‑in Mic
	Support

	Built‑in Speaker
	N/A

	WIFI
	N/A

	Network
	1 × RJ45 10 M/100 M Base‑TX Ethernet

	Video Output
	N/A

	Certification

	Protection
	IP67 (IEC 60529)

	EMC
	CE‑EMC (EN 55032, EN 61000‑3‑3, EN IEC 61000‑3‑2, EN 50130‑4)
FCC (FCC 47 CFR part15 B)

	Safety
	CE‑LVD (EN 62368‑1)

	Environment
	CE‑RoHS (2011/65/EU ; (EU) 2015/863) ; WEEE (2012/19/EU)

	General

	Power
	PoE (IEEE 802.3af)

	Power Consumption
	Max. 2.7 W

	Power Interface
	N/A

	Dimensions
	139.7 mm × 61.2 mm × 65.4 mm (5.5" × 2.4" × 2.6") (L × W × H)

	Weight
	0.15 kg (0.33 lb)

	Material
	Plastic

	Working Environment
	‑30 ℃ to 60 ℃ (‑22 ℉ to 140 ℉), Humidity: ≤ 95% RH (non‑condensing)

	Storage Environment
	‑30 ℃ to 60 ℃ (‑22 ℉ to 140 ℉), Humidity: ≤ 95% RH (non‑condensing)

	Surge Protection
	4 KV

	Reset Button
	N/A

	Web Client Language
	1 Language: English


Dimensions	
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Accessories	
	TR-JB05-A-IN
	TR-UP06-B-IN
	TR-A01-IN

	[bookmark: _GoBack]Small Bullet Junction Box(Support wiring from behind,Square)
	Bullet Pole Mounting Bracket
	NPT 3/4'' Waterproof Cable Gland
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	TR-UP06-C-IN-V2
	TR-UC08-C-V2
	

	Pole Mounting Bracket for Bullet Junction Box Only
	Bullet&Dome Corner Mounting Bracket
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	Zhejiang Uniview Technologies Co., Ltd.
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	http://www.uniview.com
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	overseasbusiness@uniview.com; globalsupport@uniview.com
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	No. 369, Xietong Road, Xixing Sub-district, Binjiang District, Hangzhou City, 310051, Zhejiang Province, China
	

	©2026 Zhejiang Uniview Technologies Co., Ltd. All rights reserved.
*Product specifications and availability are subject to change without notice.
Despite our best efforts, technical or typographical errors may exist in this document. Uniview cannot be held responsible for any such errors and reserves the right to change the contents of this document without prior notice.
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